// Events
Status on start
Login as:
Login incorrect
Reset
Restart - Reset
 - Switched off -
Firmware upgrade
HTML upgrade
Timer skiped
Clock set from NTP
Clock synchronized 
Setting changed 
Logout
Backup loaded
Backup discarded

Keepalive overflow
Sending WOL
Email started
Email sent
sending ping
Ping response
Ping unanswered




on from browser
off from browser
on from program
off from program
switched on
switched off
on from IO
off from IO
on from sensor
off from sensor
on at boot
on IO
off IO
on IO
off IO
sundial sunset
sundial sunrise
off - keepalive
on - keepalive
on - countdown
off - countdown
off pulse
on pulse
on from thermostat
off from thermostat
on Taster
off Taster
Blinking started
Blinking finished


Measurement
Voltage Sag Event
Voltage Surge Event
Over Current Event
Overpower Event
Over Frequency Event
Under Frequency Event

Voltage Sag Clear
Voltage Surge Clear
Over Current Clear
Over PowerClear
Over frequency Clear
Under Frequency Clear







// Strings
Net-PwrCtrl
 - Temp.= 
° C
 - SMTP test successful.
Message from Net-PwrCtrl
It is a test ...
Date
Relay
Action
IP of Users
Mail No.:
Su.
Mo.
Tu.
We.
Th.
Fr.
Sa.


Timer 1 start
Timer 2 start
Timer 3 start
Timer 4 start
Timer 1 end
Timer 2 end
Timer 3 end
Timer 4 end


Temperature
Humidity
Brightness

// The empty lines do not delete! New line = new record.
// Line = max. 62 characters
// If you change the text we recommends to maintain the length.
