| °C |  |
Compensation for Frequency |  |  |
Compensation for Current |  |  |
Compensation for Power |  |  |
| Hz |  |
3. Gain ( PF = 1)
Calibration Voltage | V |  |
Calibration Current | A |
Calibration Active Power | W |
Gain Voltage RMS |  |  | 20000 < x < 65535
Gain Current RMS |  |  |
Gain Active Power |  |  |
Range | 0x |  |  | 13.0D.11 Po.Cu.Vo
Offset Current RMS |  |  |
Offset Active Power |  |  |
DC Offset Current |  |  |
4. Cos φ ( PF < |1|)
Phase Compensation |  |  |
Calibration cos φ |
cos φ |  |
5. Reactive Gain ( PF < |1|)
Calibration Reactive Power | VAR |  |
Gain Reactive Power |  |  |
Offset Reactive Power |  |  |
Select a file: |  | -
⇒

System Version |  |  |
Device Address |  |  |
System Configuration | 0x |  |  | 3000000
System Status |  |  |
Thermistor Voltage |  |  |
Apparent Power Divisor |  |  | 3 (10N)
Accumulation Interval |  |  |
Event Mask Critical | 0b |  |  |
Event Mask Standard | 0b |  |  |
DIO Configuration | 0b |  |  |