Quick-Start NET-PwrCtrl
Installation:
Connect the network cable. Connect the NET-PwrCtrl to the mains. The LED flashes rapidly for the first 3 seconds and then at the secondary speed. Since most networks have a DHCP server (also available in a DSL router), the network setting is automated. Start the Internet Browser with address: http://net-control User: admin Password: anel If the NET-PwrCtrl does not show up, please check whether DHCP server is present in the network or continue with the instructions "Without DHCP". The program NET-PwrCtrl Discoverer.exe searches for all NET-PwrCtrl on the network.
With DHCP | Without DHCP
Since most networks have a DHCP server (also available in a DSL router), the network setting is automated. After switching on the NET-PwrCtrl, the DHCP function ensures that all the necessary parameters are included in the NET-PwrCtrl. The NET-PwrCtrl can now be accessed via browser with the address: http://net-control | Connect the NET-PwrCtrl and assign the following parameters to the network card: IP: 192.168.0.1; Subnet Mask: 255.255.255.0. The NET-PwrCtrl can now be accessed via browser with the address: http://192.168.0.244 or http://net-control and set as required.